YES

Force the upper bits to 0

And display the value

No

No

Is the Load button pushed?

Swap the nibbles and use XOR to toggle the two lower bits of porta for the LEDs.

YES

Is the select button pushed?

Initialize ports for input and output

Set the initial outputs for the flip-flop and the LEDs.

Start